# Plan for new buoys

A black round object with a stick

Description automatically generated

End cap - Geberit PE Enddeckel

<https://bit.ly/gerberitenddeckel>

d = (matching the tube)

A black pipe with a cross between it

Description automatically generated

Pipe - Geberit PE Pipe

<https://bit.ly/Geberit_Rohr>

363.000.16.0

d = 56 mm

Screw cap - Geberit PE threaded socket screw cap

A black plastic cap with a white background

Description automatically generated <https://bit.ly/geberitdeckel>

d = (fit the tube)

Total length = 170 cm

# A yellow and black striped pole on a grey raft Description automatically generatedContent

Foam out (possibly push in) + mill out space for sand.

**Required cavity for sand** = 1/3

**Weight for sand** = x? kg

# Colour marking

With yellow/ orange tape + reflector tape.

On the lowest ring is the marking of the club.